|  |  |  |  |
| --- | --- | --- | --- |
|  | |  | | --- | | **Simulation of Waxo\_C2**  **Date: Tuesday, May 9, 2017 Designer: Solidworks**  **Study name: Static 2**  **Analysis type: Static** | | Table of Contents  [Description 1](#_Toc482116910)  [Assumptions 2](#_Toc482116911)  [Model Information 2](#_Toc482116912)  [Study Properties 3](#_Toc482116913)  [Units 3](#_Toc482116914)  [Material Properties 4](#_Toc482116915)  [Loads and Fixtures 5](#_Toc482116916)  [Connector Definitions 5](#_Toc482116917)  [Contact Information 6](#_Toc482116918)  [Mesh information 7](#_Toc482116919)  [Sensor Details 8](#_Toc482116920)  [Resultant Forces 9](#_Toc482116921)  [Beams 9](#_Toc482116922)  [Study Results 10](#_Toc482116923)  [Conclusion 12](#_Toc482116924) | |
| Description No Data |

|  |  |  |
| --- | --- | --- |
| Assumptions  |  |  | | --- | --- | | Original Model | Model Analyzed | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model Information  |  |  |  |  |  | | --- | --- | --- | --- | --- | | |  | | --- | |  |   ****Model name:** Waxo\_C2**  ****Current Configuration:** Default** | | | | | ****Solid Bodies**** | | | | | ****Document Name and Reference**** | ****Treated As**** | ****Volumetric Properties**** | ****Document Path/Date Modified**** | | **Cut-Extrude2** | **Solid Body** | ****Mass:0.00710912 kg****  ****Volume:2.78789e-006 m^3****  ****Density:2550 kg/m^3****  ****Weight:0.0696694 N**** | ****Z:\Research project\myWork\Design\WaxoDesign\curvedBarRight.SLDPRT****  **May 05 15:40:53 2017** | | **Split Line1** | **Solid Body** | ****Mass:0.0164897 kg****  ****Volume:6.46655e-006 m^3****  ****Density:2550 kg/m^3****  ****Weight:0.161599 N**** | ****Z:\Research project\myWork\Design\WaxoDesign\torqueBar.SLDPRT****  **May 05 15:40:54 2017** | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Study Properties  |  |  | | --- | --- | | Study name | Static 2 | | Analysis type | Static | | Mesh type | Solid Mesh | | Thermal Effect: | On | | Thermal option | Include temperature loads | | Zero strain temperature | 298 Kelvin | | Include fluid pressure effects from SOLIDWORKS Flow Simulation | Off | | Solver type | FFEPlus | | Inplane Effect: | Off | | Soft Spring: | Off | | Inertial Relief: | Off | | Incompatible bonding options | Automatic | | Large displacement | Off | | Compute free body forces | On | | Friction | Off | | Use Adaptive Method: | Off | | Result folder | SOLIDWORKS document (Z:\Research project\myWork\Design\WaxoDesign) | |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Units  |  |  | | --- | --- | | Unit system: | SI (MKS) | | Length/Displacement | mm | | Temperature | Kelvin | | Angular velocity | Rad/sec | | Pressure/Stress | N/m^2 | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Material Properties  |  |  |  | | --- | --- | --- | | ****Model Reference**** | ****Properties**** | ****Components**** | |  | |  |  | | --- | --- | | ****Name:**** | **Std CF** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Max von Mises Stress** | | ****Yield strength:**** | **2.75e+009 N/m^2** | | ****Tensile strength:**** | **1.95e+009 N/m^2** | | ****Compressive strength:**** | **4e+009 N/m^2** | | ****Elastic modulus:**** | **7e+010 N/m^2** | | ****Poisson's ratio:**** | **0.21** | | ****Mass density:**** | **2550 kg/m^3** | | ****Shear modulus:**** | **3e+010 N/m^2** | | **SolidBody 1(Cut-Extrude2)(curvedBarRight-1),**  **SolidBody 1(Split Line1)(torqueBar-2)** | | **Curve Data:N/A** | | | |  | |  |  | | --- | --- | | ****Name:**** | **E fiberglass** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Max von Mises Stress** | | ****Yield strength:**** | **1.95e+009 N/m^2** | | ****Tensile strength:**** | **2.75e+009 N/m^2** | | ****Compressive strength:**** | **4e+009 N/m^2** | | ****Elastic modulus:**** | **7e+010 N/m^2** | | ****Poisson's ratio:**** | **0.21** | | ****Mass density:**** | **2550 kg/m^3** | | ****Shear modulus:**** | **3e+010 N/m^2** | | **<Material\_ComponentList1/>** | | **Curve Data:N/A** | | | |  | |  |  | | --- | --- | | ****Name:**** | **6061 Alloy** | | ****Model type:**** | **Linear Elastic Isotropic** | | ****Default failure criterion:**** | **Max von Mises Stress** | | ****Yield strength:**** | **5.51485e+007 N/m^2** | | ****Tensile strength:**** | **1.24084e+008 N/m^2** | | ****Elastic modulus:**** | **6.9e+010 N/m^2** | | ****Poisson's ratio:**** | **0.33** | | ****Mass density:**** | **2700 kg/m^3** | | ****Shear modulus:**** | **2.6e+010 N/m^2** | | ****Thermal expansion coefficient:**** | **2.4e-005 /Kelvin** | | **<Material\_ComponentList1/>** | | **Curve Data:N/A** | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Loads and Fixtures**  | ****Fixture name**** | ****Fixture Image**** | ****Fixture Details**** | | --- | --- | --- | | **Fixed-1** |  | |  |  | | --- | --- | | Entities: | **2 face(s)** | | Type: | **Fixed Geometry** | | | ****Resultant Forces****   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Components** | **X** | **Y** | **Z** | **Resultant** | | **Reaction force(N)** | **-195.455** | **-0.0547009** | **41.5561** | **199.824** | | **Reaction Moment(N.m)** | **0** | **0** | **0** | **0** | | | |  | ****Load name**** | ****Load Image**** | ****Load Details**** | | --- | --- | --- | | **Force-2** |  | |  |  | | --- | --- | | Entities: | **1 face(s), 1 plane(s)** | | Reference: | **PLANE1** | | Type: | **Apply force** | | Values: | **195.6, 41.6, --- N** | | |

|  |
| --- |
| Connector Definitions No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Contact Information  | Contact | Contact Image | Contact Properties | | --- | --- | --- | | Global Contact |  | |  |  | | --- | --- | | Type: | **Bonded** | | Components: | **1 component(s)** | | Options: | **Compatible mesh** | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Mesh information  |  |  | | --- | --- | | Mesh type | Solid Mesh | | Mesher Used: | Standard mesh | | Automatic Transition: | Off | | Include Mesh Auto Loops: | Off | | Jacobian points | 4 Points | | Element Size | 4.43824 mm | | Tolerance | 0.221912 mm | | Mesh Quality | High | | Remesh failed parts with incompatible mesh | Off |  Mesh information - Details  |  |  | | --- | --- | | Total Nodes | 4198 | | Total Elements | 1750 | | Maximum Aspect Ratio | 10.864 | | % of elements with Aspect Ratio < 3 | 73.7 | | % of elements with Aspect Ratio > 10 | 0.0571 | | % of distorted elements(Jacobian) | 0 | | Time to complete mesh(hh;mm;ss): | 00:00:02 | | Computer name: | ASUS-YACINE | |  | | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Sensor Details  | Sensor name | Location | Sensor Details | | --- | --- | --- | | Stress1 |  | Value : 1166.37 N/mm^2 (MPa)  Entities :  Result :Stress  Component :VON: von Mises Stress  Criterion :Model Max  Step Criterion : Across all Steps  Step No.:1  Alert Value: is greater than 1e+009 N/mm^2 (MPa) | | Mass1 |  | Value : 72.0092389 g  Entities :2 component(s)  Result :Stress  Component :VON: von Mises Stress  Criterion :Model Max  Step Criterion : Across all Steps  Step No.:1  Alert Value: NA | | Stress2 |  | Value : 169168 psi  Entities :  Result :Stress  Component :VON: von Mises Stress  Criterion :Model Max  Step Criterion : Across all Steps  Step No.:1  Alert Value: NA | | Minimum Factor of Safety1 |  | Value : 1.39641  Entities :  Result :Factor of Safety  Component :Automatic  Criterion :Model Max  Step Criterion : Across all Steps  Step No.:1  Alert Value: NA | | Mass2 |  | Value : 931.539708 g  Entities :  Result :Stress  Component :VON: von Mises Stress  Criterion :Model Max  Step Criterion : Across all Steps  Step No.:1  Alert Value: NA | |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Resultant ForcesReaction forces  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N | -195.455 | -0.0547009 | 41.5561 | 199.824 |  Reaction Moments  | Selection set | Units | Sum X | Sum Y | Sum Z | Resultant | | --- | --- | --- | --- | --- | --- | | Entire Model | N.m | 0 | 0 | 0 | 0 | |
|  |

|  |
| --- |
| Beams No Data |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Study Results  | Name | Type | Min | Max | | --- | --- | --- | --- | | Stress1 | VON: von Mises Stress | 32941.4 N/m^2  Node: 3833 | 1.16637e+009 N/m^2  Node: 3411 | | **Waxo\_C2-Static 2-Stress-Stress1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Displacement1 | URES: Resultant Displacement | 0 mm  Node: 33 | 102.907 mm  Node: 3137 | | **Waxo\_C2-Static 2-Displacement-Displacement1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Strain1 | ESTRN: Equivalent Strain | 4.16573e-007  Element: 1624 | 0.0118756  Element: 1430 | | **Waxo\_C2-Static 2-Strain-Strain1** | | | |  | Name | Type | Min | Max | | --- | --- | --- | --- | | Factor of Safety1 | Max von Mises Stress | 1.39641  Node: 17 | 59196  Node: 3833 | | **Waxo\_C2-Static 2-Factor of Safety-Factor of Safety1** | | | | |

|  |
| --- |
| Conclusion |